Beware SX-2 users!

In order to get sound working on Carnivore2 cartridges running firmware 2.50 or newer you need to set "Dual-Reset" feature "ON" within Carnivore configuration menu. This is done by pressing "C" at the startup menu and then toggling the option to "Y". Then exit the configuration menu with "ESC".

8Bits4Ever Team